Old vs. New SelectorsSelectorOld

esNew Value ddresssingl st, wildcar ngesingle,

, wildcardT ort Protoco le, list, r ingleIPSec colsingle,

ELETEDPort ssingle, li ildcardsing ildcard, ra v4 TOSsingl ldcardDELET

6 Classsing ildcardDELE v6 Flow Lab gle, wildca

ETEDUser ID e, list, wi dsingleSecu

Labelsingl le

Required IPsec CombinationsnTransport ModeuAHuESPuAH+ESPnTunnel ModeuAHuESPnNo requirement to support nested SAs originating and terminating at the same endpointsnThe only ordering in an SA bundle is explicitly AH then ESP in transport mode

SA Termination Examples

Host orGatewayHost orGatewayHostGatewayHost