\hsize=4in\parindent=0\parskip=.1666in
\def\num#1{\strut\llap{#1.\quad}}
How to log in to Athena from this terminal:

\parskip=0pt
\num{1}Turn on modem (slide switch on top)

\num{2}Turn on terminal (toggle switch; left back)

\num{3}The terminal will beep obnoxiously.  Hit SET-UP.

\num{4}Press 5, then hit 7 and 8 until both ``T SPEED'' and ``R SPEED'' are
set to 1200 baud.

\num{5}Use the arrow keys $\leftarrow$ and $\rightarrow$ to move the cursor
over the numbers at the bottom, and use the 6 key to toggle them between 1
and 0.  The correct settings are

\medskip
\centerline{1 0101  2 0*11  3 0100  4 0010}

\medskip
Where the * is 0 for no key click and 1 for key click.  Do not hit 1 or 0,
as these reset the procedure.  Don't complain to me, that's DEC's fault.

\num{6}You can use the $\uparrow$ and $\downarrow$ keys to adjust the
brightness of the screen.

\num{7}Hit SET-UP again and type AT DT87227 and press RETURN.  If you get
a busy signal try AT DT87472.

\num{8}You will be asked for MACHINE NAME.  Type ``dialup'' (all lowercase)
and hit RETURN.

\num{9}You can now log in as usual.  You only have one window, and it can't
do graphics or Zephyr, but it's the best we can do.

\num{10}When you are done, be sure to turn off the modem, the terminal, any
fans that you may have turned on (they're to your right), and turn off the
lights on your way out.

\end
