Input When Gateway gets an RIP input packet it dispatches to rip in proce- dure which does the following: if the source address of the packet is one of our address on the incom- ming net, or if the net has IF RIP IGN set the packet is ignored. if the version �eld is not the packet is ignored. dispatches if the packet contains request RIP REQUES or RIP REQGW ), logs an error if it is either TRACE ON or trace off Otherwise the routing table is updated as follows (for each netinfo structur in the packet): if the destination address equals (default), the route is ignored. if the metric is greater than i.e. 16) or less than 0, it is set to the routing table entry for the destination is lookuped up, creat- ing if necessary If the entry is created its metric is set to if it already exists with metric of the route is ignored.