/CE on D2A

Accumulator Output X 0 orig orig+shifted

Accumulator Load

Accumulator Clear

Data Bus A2D data SRAM data

Address Bus sampctr shiftctr

/OE on SRAM

/WE on SRAM shiftbuf

STATUS on A2D

R/W on A2D

SAMPCLK CLK