DRAM /RAS

DRAM address bus 0 0 0 1 17 8 (Columns) 8 9 (Columns) 9 10 (Columns) 10 11 (Columns)(Columns)

Column-counter OE

Column-counter /CLR

Row-counter /OE

Row-counter /CLR

Row-counter CLK

HDRIVE

VDRIVE

CSYNC

CBLANK