This paper reflects work done on, and is applicable to, acetate film base only. It does not apply to modern polyester film base.

This paper was originally published in the June

1965 issue of the Journal of the Society of Motion

Picture and Television Engineers, and is

reproduced here with permission.

Society of Motion Picture and Television Engineers 595 Hartsdale Avenue White Plains, New York 10607 www.smpte.org