PostScript Processing speed test � Test executed on: Unknown device Running Adobe PostScript �

The white area around the border shows your printer’s dead-zone.

The numbers printed represent a relative index to the first widely used PostScript printer, the Apple LaserWriter. If the numbers under the "This Printer" column indicate a 1.0, then your printer is as fast as an Apple LaserWriter. If the bottom number is 5.0, then it is 5 times faster than the Apple LaserWriter. Lastly, if the number is less than one, for example 0.8, then your printer is slower than the Apple LaserWriter. The numbers in each row have this meaning:

PPST-G is for graphics speed, PPST-R is for RAM & cache speed, PPST-M is for mathematics speed, PPST-I is for bitmapped image speed and PPST, the last row, is for the overall speed rating. Note that the overall speed rating is not an average but is based on the time of all the tests added together.

The actual number of seconds of execution for each test is as follows: 0 seconds for PPST-G, 0 seconds for PPST-R, 0 seconds for PPST-M, 0 seconds for PPST-I, and 0 seconds for the entire test, or PPST for short.

by Jean-Serge Gagnon <JSG8A@ACADVM1.UOTTAWA.CA> Computer Hardware Maintenance Specialist 222 Jean Perrin Gatineau, Quebec, Canada J8V 2R4

613-791-0785 March 9th, 1994

PPST index results

index

PPST-G PPST-R PPST-M PPST-I

PPST

Apple LaserWriter 1.0 1.0 1.0 Next ver 1.0

Apple LaserWriter II NTX ..8 ..0 ..9 Next ver ..3

QMS PS 2000

.34.6 .6.0 .3.0 Next ver

.7.4

This printer

too fast! too fast! too fast! Next ver

too fast!