\HeaderA{stormer}{The Stormer Viscometer Data}{stormer}
\keyword{datasets}{stormer}
\begin{Description}\relax
The stormer viscometer measures the viscosity of a fluid by measuring the
time taken for an inner cylinder in the mechanism to perform a fixed number
of revolutions in response to an actuating weight.  The viscometer is
calibrated by measuring the time taken with varying weights while the
mechanism is suspended in fluids of accurately known viscosity.  The data
comes from such a calibration, and theoretical considerations suggest a
nonlinear relationship between time, weight and viscosity, of the form
\code{Time = (B1*Viscosity)/(Weight - B2) + E}
where \code{B1} and \code{B2}
are unknown parameters to be estimated, and \code{E} is error.
\end{Description}
\begin{Usage}
\begin{verbatim}
stormer
\end{verbatim}
\end{Usage}
\begin{Format}\relax
The data frame contains the following components:
\describe{
\item[\code{Viscosity}] Viscosity of fluid

\item[\code{Wt}] Actuating weight

\item[\code{Time}] Time taken
}
\end{Format}
\begin{Source}\relax
E. J. Williams (1959)
\emph{Regression Analysis.}
Wiley.
\end{Source}
\begin{References}\relax
Venables, W. N. and Ripley, B. D. (2002)
\emph{Modern Applied Statistics with S.} Fourth edition.  Springer.
\end{References}

