\HeaderA{system.time}{CPU Time Used}{system.time}
\aliasA{unix.time}{system.time}{unix.time}
\keyword{utilities}{system.time}
\begin{Description}\relax
Return CPU (and other) times that \code{expr} used.
\end{Description}
\begin{Usage}
\begin{verbatim}
system.time(expr, gcFirst = TRUE)
unix.time(expr, gcFirst = TRUE)
\end{verbatim}
\end{Usage}
\begin{Arguments}
\begin{ldescription}
\item[\code{expr}] Valid \R{} expression to be \dQuote{timed}
\item[\code{gcFirst}] Logical - should a garbage collection be performed
immediately before the timing?  Default is \code{TRUE}.
\end{ldescription}
\end{Arguments}
\begin{Details}\relax
\code{system.time} calls the builtin \code{\LinkA{proc.time}{proc.time}},
evaluates \code{expr}, and then calls \code{proc.time} once more,
returning the difference between the two \code{proc.time} calls.

\code{unix.time} is an alias of \code{system.time}, for
compatibility reasons.

Timings of evaluations of the same expression can vary considerably
depending on whether the evaluation triggers a garbage collection. When
\code{gcFirst} is \code{TRUE} a garbage collection (\code{\LinkA{gc}{gc}})
will be performed immediately before the evaluation of \code{expr}.
This will usually produce more consistent timings.
\end{Details}
\begin{Value}
A numeric vector of length 5 containing the user cpu, system cpu, elapsed,
subproc1, subproc2 times. The subproc times are the user and
system cpu time used by child processes (and so are usually zero).

The resolution of the times will be system-specific; it is common for
them to be recorded to of the order of 1/100 second, and elapsed
time is rounded to the nearest 1/100.
\end{Value}
\begin{Note}\relax
It is possible to compile \R{} without support for \code{system.time},
when the function will throw an error.
\end{Note}
\begin{SeeAlso}\relax
\code{\LinkA{proc.time}{proc.time}}, \code{\LinkA{time}{time}} which is for time series.
\end{SeeAlso}
\begin{Examples}
\begin{ExampleCode}
require(stats)
system.time(for(i in 1:100) mad(runif(1000)))
## Not run: 
exT <- function(n = 1000) {
  # Purpose: Test if system.time works ok;   n: loop size
  system.time(for(i in 1:n) x <- mean(rt(1000, df=4)))
}
#-- Try to interrupt one of the following (using Ctrl-C / Escape):
exT()                 #- about 3 secs on a 1GHz PIII
system.time(exT())    #~ +/- same
## End(Not run)\end{ExampleCode}
\end{Examples}

